  UART cable:
1. Phone must be powered on.
2. Connect the phone to UART cable.
3. Choose correct COM port in port settings.
4. Check security type ("Old Security" or "New Security").
5. Fill values what you need to repair.
6. Press "Repair" button.
  USB cable with "Old Security" option:
1. Phone must be powered on.
2. Type *#782872# to switch phone to Qualcomm USB mode,
   (after operations you can enter *#726872# to switch back to Samsung USB mode.)
3. Connect USB cable, install drivers.
4. Select diagnostic port in port settings.
5. Fill values what you need to repair.
6. Press "Repair" button.
If you got "Calculating ... error" or "Reading sysinfo ... access denied" errors,
then you must check "New security" option.
  USB cable with "New Security" option:
1. Phone must be powered on.
2. Type *#726872# to switch phone to Samsung USB mode.   
3. Connect USB cable, install drivers.
4. Fill values what you need to repair.
5. Press "Repair" button.