1. Choose correct flash file(s).
2. Choose flash option if needed:
   -"Re-write NV" - Warning! This option will erase all calibration data!
   -"Single file firmware" - if you have *.pac firmware
3. Press "Flash" button.
4. Connect phone in flash mode (Press "1" button and connect USB cable).