  UART cable:
1. Phone must be powered on.
2. Connect the phone to UART cable.
3. Choose correct COM port in port settings.
4. Press "Unlock" button for direct unlock or "Read codes" to read security codes.
  USB cable:
1. Phone must be powered on.
2. Type *#782872# to switch phone to Qualcomm USB mode,
   (after operations you can enter *#726872# to switch back to Samsung USB mode.)
3. Connect USB cable, install drivers.
4. Select diagnostic port in port settings.
5. Press "Unlock" button for direct unlock or "Read codes" to read security codes.