1. Phone must be powered on.
2. Connect the phone to UART cable.
3. Choose correct COM port in port settings
4. Fill values what you need to repair.
5. Press "Repair" button.
6. If you have connection errors, try to type *#197328640#, 
    select: Common - Diag Config - UART_diag USB_NULL and reboot phone.