  UART cable:
1. Phone must be powered on.
2. Connect the phone to UART port.
3. Choose correct COM port in port settings.
4. Press "Unlock" button for direct unlock or "Read codes" to read security codes.
    Or you can "Read User Lock" or "Reset User Lock".
  USB cable:
1. Phone must be powered on.
2. Type *#7284# and choose phone USB.
3. Type *#197328640#, select: Common - Diag Config - USB diag.
4. Reboot phone.
5. Connect USB cable, install drivers.
6. Select diagnostic port in port settings.
7. Press "Unlock" button for direct unlock or "Read codes" to read security codes.
    Or you can "Read User Lock" or "Reset User Lock".