  UART cable:
1. Phone must be powered on.
2. Connect the phone to UART cable.
3. Choose correct COM port in port settings
4. Fill values what you need to repair.
5. Press "Repair" button.
  USB cable:
1. Phone must be powered on.
2. Type *#7284# and choose USB Configuration - USB-Phone(Modem).
3. Type *#9090#, select: UART_HFK USB_DIAG.
4. Reboot phone.
5. Connect USB cable, install drivers.
6. Select diagnostic port in port settings.
7. Fill values what you need to repair.
8. Press "Repair" button.