1. Choose correct flash file(s).
2. Choose flash option if needed (Erase all flash).
 Warning!This option will erase all calibration data!
3. Press "Flash" button.
4. Connect phone in flash mode:
- (Disconnect battery and connect USB cable, insert battery after
connecting.)
- (Or disconnect battery, press vol.down and connect USB cable, insert
battery after connecting).