  UART cable:
1. Phone must be powered on.
2. Connect the phone to UART cable.
3. Choose correct COM port in port settings.
4. Fill values what you need to repair.
5. Press "Repair" button.
  USB cable:
1. Phone must be powered on.
2. Type *#782872# to switch phone to Qualcomm USB mode,
   (after operations you can enter *#726872# to switch back to Samsung USB mode.)
3. Connect USB cable, install drivers.
4. Select diagnostic port in port settings.
5. Fill values what you need to repair.
6. Press "Repair" button.